ITEM 154.02 SAND BORROW CUBIC YARD

GENERAL

The work under this item shall consist of furnishing, placing, and compacting Sand Borrow at locations specified on the Plans and as required by the Engineer.

MATERIALS

Sand shall consist of clean, inert, hard, durable grains of quartz or other hard durable rock, free from loam or clay, surface coating, and deleterious materials. Sand shall conform to the Massachusetts Department of Transportation Standard Specifications for Highways and Bridges Division III, M1.04.1, Sand Borrow for Subdrains for Type b material.

METHOD OF MEASUREMENT

Sand Borrow will be measured for payment by the cubic yard, complete in place.

BASIS OF PAYMENT

Sand Borrow will be paid for at the contract unit price per cubic yard, which price shall include all labor, materials, equipment, and incidental costs required to complete the work.