ITEMS 245.12 PRECAST CONCRETE END SECTION EACH

FOR 12 INCH TRENCH DRAIN

GENERAL

This work shall consist of furnishing and placing concrete end sections for Trench Drains as specified on the Plans and as required by the Engineer.

MATERIALS

Concrete shall conform to the Massachusetts Department of Transportation Standard Specifications for Highways and Bridges Division III, M4.02.14 Precast Concrete Highway Units.

Steel shall conform to the Massachusetts Department of Transportation Standard Specifications for Highways and Bridges Division III, M8.01.

METHOD OF MEASUREMENT

Precast Concrete End Section will be measured for payment by the each, complete in place.

BASIS OF PAYMENT

Precast Concrete End Section will be paid for at the contract unit price per each, which price shall include all labor, materials, equipment, and incidental costs required to complete the work. No separate payment will be made for excavation or connections to the trench drain, but all costs in connection therewith shall be included in the Contract unit price bid.

Gravel base will be paid for separately under Item 151.02, Gravel.