ITEM 251.708 8 INCH SOLID PVC PIPE LINEAR FOOT

ITEM 251.712 12 INCH SOLID PVC PIPE LINEAR FOOT

ITEM 251.724 24 INCH SOLID PVC PIPE LINEAR FOOT

GENERAL

The work under this item shall consist of furnishing, placing and backfilling solid wall polyvinylchloride (PVC) drainage pipes as part of green infrastructure components.

PVC pipe shall be as specified and installed as required by the Boston Water and Sewer Commission Standard Specifications.

METHOD OF MEASUREMENT

8 Inch Solid PVC Pipe will be measured for payment by the linear foot, complete in place. No deductions shall be made for the length of wye-branches or other fittings.

12 Inch Solid PVC Pipe will be measured for payment by the linear foot, complete in place. No deductions shall be made for the length of wye-branches or other fittings.

24 Inch Solid PVC Pipe will be measured for payment by the linear foot, complete in place. No deductions shall be made for the length of wye-branches or other fittings.

BASIS OF PAYMENT

8 Inch Solid PVC Pipe will be paid for at the Contract unit price per linear foot which price shall include all labor, materials, equipment, and incidental costs necessary to complete the work. No separate payment will be made for excavation, furnishing and installing (including joining) pipe and fittings (including but not limited to wyes, tees, and couplings), and furnishing, placing, and compacting backfill material, but all costs in connection therewith shall be included in the Contract unit price bid.

12 Inch Solid PVC Pipe will be paid for at the Contract unit price per linear foot which price shall include all labor, materials, equipment, and incidental costs necessary to complete the work. No separate payment will be made for excavation, furnishing and installing (including joining) pipe and fittings (including but not limited to wyes, tees, and couplings), and furnishing, placing, and compacting backfill material, but all costs in connection therewith shall be included in the Contract unit price bid.

24 Inch Solid PVC Pipe will be paid for at the Contract unit price per linear foot which price shall include all labor, materials, equipment, and incidental costs necessary to complete the work. No separate payment will be made for excavation, furnishing and installing (including joining) pipe and fittings (including but not limited to wyes, tees, and couplings), and furnishing, placing, and compacting backfill material, but all costs in connection therewith shall be included in the Contract unit price bid.